{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[2,2,2,5],[3,2,3,5],[4,2,4,5],[5,2,5,5]]}
["Entstehende Kräfte beim Abrutschen einer Last"]
[]
["dS=",3.5,"Durchbiegung der Doppelbodenplatte\nHolzwerkstoffplatte: Etwa 3,5 mm\nCalziumsulfatplatte: Etwa 2,5 mm"]
["h=",50,"Fallhöhe"]
["m=",300,"Masse der abrutschenden Last"]
["g=",9.8070000000000004,"Gravitationskonstante"]
[]
[null,null,"V=",{"$f":"SQRT(2*B6*B4/1000)","v":0.99030298393976379},{"$f":"D8*3.6","v":3.5650907421831497}]
[]
[]
[]
[null,null,"F=",{"$f":"(B5*B6*B4/1000)/(B3/1000)","v":42029.999999999993},{"$f":"D12/1000","v":42.029999999999994}]
[]
[]
[]
[]
[]
[]
[null,null,"t=",{"$f":"D8/B6","v":0.10097919689403118}]